{"name":"ag-lcd","vers":"0.3.0","deps":[{"name":"embedded-hal","req":"^1.0.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"port-expander","req":"^0.6.2","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"shared-bus","req":"^0.2","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"ufmt","req":"^0.1.0","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"28a8677258eb556ffe8eacb10f23f004a70107aab77a769aa15a2435473f46e7","features":{"avr-hal":[],"i2c":["port-expander"]},"yanked":false}
