{"name":"arduino_nano33iot","vers":"0.8.0","deps":[{"name":"atsamd-hal","req":"^0.23.0","features":["undoc-features"],"optional":false,"default_features":false,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"cortex-m-rt","req":"^0.7","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"rand","req":"^0.8","features":["small_rng"],"optional":false,"default_features":false,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"usb-device","req":"^0.3.2","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"cortex-m","req":"^0.7","features":["critical-section-single-core"],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-graphics","req":"^0.7","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"panic-halt","req":"^1.0.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"panic-semihosting","req":"^0.6","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"ssd1306","req":"^0.7","features":["graphics"],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"st7735-lcd","req":"^0.8","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"usbd-serial","req":"^0.2.2","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"8c8af64516815469270cf60ed6858c4e154be391cc3d41864056055cd9043a9f","features":{"default":["rt","atsamd-hal/samd21g"],"rt":["cortex-m-rt","atsamd-hal/samd21g-rt"],"usb":["atsamd-hal/usb","usb-device"],"use_semihosting":[]},"yanked":false}
