{"name":"adafruit-seesaw","vers":"0.13.0","deps":[{"name":"defmt","req":"^1","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-hal","req":"^1.0.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"rgb","req":"^0.8.50","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"cortex-m","req":"^0.7","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"cortex-m-rt","req":"^0.7","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-hal-bus","req":"^0.3","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"heapless","req":"^0.8","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"rtt-target","req":"^0.6","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"stm32f4xx-hal","req":"^0.22","features":["stm32f405","sdio"],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"e44e1800ece3faaf2053aea66e4a33adf62a1d46112d9488651ed80cedcdd4a1","features":{"default":["device_arcade_button_1x4","device_neokey_1x4","device_neorotary4","device_neoslider","device_neotrellis","device_rotary_encoder","device_soil_sensor","module_adc","module_encoder","module_gpio","module_timer","module_touch"],"defmt":["dep:defmt"],"device_arcade_button_1x4":["module_gpio","module_timer"],"device_neokey_1x4":["module_gpio"],"device_neorotary4":["module_gpio","module_encoder"],"device_neoslider":["module_adc","module_gpio"],"device_neotrellis":["module_keypad"],"device_rotary_encoder":["module_encoder","module_gpio"],"device_soil_sensor":["module_touch"],"module_adc":[],"module_encoder":["module_gpio"],"module_gpio":[],"module_keypad":[],"module_neopixel":[],"module_timer":[],"module_touch":[],"nightly":["device_arcade_button_1x4","device_neokey_1x4","device_neorotary4","device_neoslider","device_neotrellis","device_rotary_encoder","module_keypad","module_neopixel"]},"yanked":false}
