{"name":"arduino_mkrvidor4000","vers":"0.6.1","deps":[{"name":"atsamd-hal","req":"^0.14","features":[],"optional":false,"default_features":false,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"cortex-m-rt","req":"^0.7","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"panic-halt","req":"^0.2","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"panic-semihosting","req":"^0.5","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"64639fe9dd56e5654afacf63b396c51b42a894f222d0b472d075aa44fd30159c","features":{"default":["rt","atsamd-hal/samd21g"],"rt":["cortex-m-rt","atsamd-hal/samd21g-rt"],"unproven":["atsamd-hal/unproven"],"usb":["atsamd-hal/usb"],"use_semihosting":[]},"yanked":false}
