{"name":"adafruit-lcd-backpack","vers":"0.1.2","deps":[{"name":"defmt","req":"^0.3","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-hal","req":"^0.2","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"mcp230xx","req":"^1.0.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"b058f81e3722cc1c2b7ec1399de8106fa74f107c187868cc91cad9de48db4c54","features":{"defmt":["dep:defmt"]},"yanked":false}
