{"name":"adafruit-alphanum4","vers":"0.1.2","deps":[{"name":"ascii","req":"^1.0.0","features":[],"optional":false,"default_features":false,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-hal","req":"^0.2.3","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"ht16k33","req":"^0.4.0","features":[],"optional":false,"default_features":false,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"6371bb72d395cdf08f6b6397b745894485d1e05613726b771009eee5c5c98a8a","features":{},"yanked":false}
