{"name":"arduino-wifi-tft-lcd-canvas-server","vers":"1.0.0","deps":[{"name":"byteorder","req":"^1.5","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"clap","req":"^4.5","features":["derive"],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"local-ip-address","req":"^0.6.1","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"pbr","req":"^1.1","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"45c2fab51ceba9ccc2de7ab300f1b351383760d17ba738c8fa09e22b4fc15e3d","features":{},"yanked":false}
