{"name":"alarmo","vers":"0.0.5","deps":[{"name":"cortex-m","req":"^0.7.5","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"cortex-m-rt","req":"^0.7.5","features":["set-vtor","set-sp","zero-init-ram"],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"display-interface","req":"^0.5.0","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-alloc","req":"^0.6.0","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-graphics","req":"^0.8.1","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"embedded-hal","req":"^1.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"mipidsi","req":"^0.8.0","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"stm32h7xx-hal","req":"^0.16.0","features":["stm32h735","fmc","rt"],"optional":false,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"usb-device","req":"^0.3","features":[],"optional":true,"default_features":true,"target":null,"kind":"normal","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"panic-halt","req":"^1.0.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"panic-rtt-target","req":"^0.1.0","features":["cortex-m"],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null},{"name":"usbd-serial","req":"^0.2.0","features":[],"optional":false,"default_features":true,"target":null,"kind":"dev","registry":"https://github.com/rust-lang/crates.io-index","package":null}],"cksum":"d48be96ad8f8a741439da2df1492c4db0ab019d945f4b1c219645a79278bff37","features":{"alloc":["embedded-alloc","cortex-m/critical-section-single-core"],"default":[],"display":["display-interface"],"display-mipidsi":["display","mipidsi","embedded-graphics"],"panic":["display-mipidsi"],"usb":["usb-device","stm32h7xx-hal/usb_hs"]},"yanked":false}
